Note: This IBM PC BIOS API call is for DOS/Win16 personality only. Use Family API for portability.

Note: osFree Macro Library provides macros for most of functions

@WrtTTY

Brief

Write char in TTY mode

BIOS Interrupt

INT10H: H

Family API

fapi

Syntax

@WrtTTY char, page

Parameters

char (BYTE) - character code

page (BYTE) - optional video page number

Return

none