## Physical Device Driver Reference

[prev][next][parent][TOC]

### MOU_SETMOUSTATUS (5Ch) - Status Flag

Status Flag Has the following bit-level definitions:

High Byte Bit settings are as follows:
Bits 7-2 Reserved. Set to 0.
Bit 1 Set, if mouse data returned in mickeys, not display units
Bit 0 Set, if the interrupt level pointer draw routine is not called.
Low Byte Bit settings are as follows:
Bits 7-0 Reserved. Set to 0.

A set bit has a value of 1.