## Physical Device Driver Reference

[prev][next][parent][TOC]

### 1Fh - Remarks

When a device driver receives this command, all physical device drivers have been loaded and initialized. Virtual device drivers have not been loaded and initialized. The device driver can now establish links to other physical device drivers.

The initialization complete command is sent to the device driver only if it is a level 3 device driver and if Bit 4 is set in the Capabilities Bit Strip in the device driver header. (See Capabilities Bit Strip.)

Using this command can remove any device driver ordering requirements in config.sys. (BASEDEV= and DEVICE= ).

See AttachDD for additional information on setting up IDCs with other physical device drivers.