## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### SplQueryQueue Parameter - pBuf

pBuf (PVOID) - in/out Buffer.

The returned contents of the buffer depend on the value specified in ulLevel as follows:

ulLevel Buffer Contents

3 A PRQINFO3 structure, with associated variable information up to cbBuf. The fsType bit PRQ3_TYPE_APPDEFAULT is set for the application default queue only.

4 A PRQINFO3 structure, with associated variable information, and an array of PRJINFO2 structures, one for each job in the queue, up to cbBuf.

5 A queue name of type PSZ.

6 A PRQINFO6 structure, with associated variable information up to cbBuf.

7 A PRQINFO3 structure, with associated variable information, and an array of PRJINFO4 structures, one for each job in the queue, up to cbBuf.