## Physical Device Driver Reference

[prev][next][parent][TOC]

### ASYNC_GETLINESTATUS (65h) - Transmit Status

Transmit Status Returned as bit-significant values. If the bit is 1, the condition is TRUE. If the bit is 0, the condition is FALSE. The number at the beginning of the description is the bit position number. The bit positions go from least to most significant.

Bit 0 WRITE request packets in progress or queued
Bit 1 Data in the physical device driver transmit queue
Bit 2 Transmit hardware is currently transmitting data
Bit 3 Character waiting to be transmitted immediately
Bit 4 Waiting to automatically transmit an XON
Bit 5 Waiting to automatically transmit an XOFF
Bit 6 Undefined
Bit 7 Undefined