## ALP Programming Guide and Reference

[prev][next][parent][TOC]

### Notes

Coding WAIT after an ESC instruction ensures that any unmasked floating- point exceptions the instruction may cause are handled before the processor has a chance to modify the instruction's results.

FWAIT is an alternate mnemonic for WAIT.

Refer to the Intel documentation for more information about when to use WAIT (FWAIT).