## Display Device Driver Reference for OS/2

[prev][next][parent][TOC]

### Function 100h - Remarks

The Touchxxxx fields circumscribe the area of the LVB, or PVB, for a rectangle that was potentially changed by the given operation. For example, a Write that included the cells (10,12) to (79,12), (0,13) to (79,13), and (0,14) to (8,14) returns TouchXLeft=0, TouchYTop=12, TouchXRight=79, and TouchYBottom=14. Any new functions added to the BVH interface that can affect the data in the PVB or LVB must include a return area for the rectangle of the video buffer that was affected by the given call.

The LVBxxxx fields indicate that an LVB can differ from the normal LVB format. The information about the LVB is taken from these fields, if they are included. Notice that these fields allow an LVB to begin at a location other than (0,0) and allow LVBs of different row and column dimensions.