## Virtual Device Driver Reference for OS/2

[prev][next][parent][TOC]

### VDHPopRegs Parameter - RegFlag

RegFlag (FLAGS) Flag indicating which client registers to pop.

These flags can be "ORed" together to indicate more than one register. Possible values are:

VDHREG_AX Pop the AX register
VDHREG_BX Pop the BX register
VDHREG_CX Pop the CX register
VDHREG_DX Pop the DX register
VDHREG_SI Pop the SI register
VDHREG_DI Pop the DI register
VDHREG_BP Pop the BP register
VDHREG_SP Pop the SP register
VDHREG_DS Pop the DS register
VDHREG_ES Pop the ES register
VDHREG_SS Pop the SS register
VDHREG_FLAG Pop the Flags register
VDHREG_ALL Pop all the registers
VDHREG_GENERAL Pop all the registers except SS and SP