## Virtual Device Driver Reference for OS/2

[prev][next][parent][TOC]

### Input/Output Port Support

The virtual CMOS device driver component monitors all accesses to its two DOS session I/O ports. The two ports are a write-only address latch and a read/write data latch. The address latch port has two functions, NMI Disable and CMOS/RTC Device Address Selection. The data latch is a register for holding a byte being transferred to or from the CMOS/RTC device.