## Virtual Device Driver Reference for OS/2

[prev][next][parent][TOC]

### Real-Time Clock and Interrupt Access

The Real-Time Clock consists of a time-of-day clock, an alarm interrupt, and a periodic interrupt. Accesses to the Real-Time Clock to change the time of day or the timing mode, or to set an alarm or periodic interrupt, are disallowed. The CMOS/RTC registers related to the Real-Time Clock are supported for read-only access. Because interrupts can only be supported through write access to the ports, Real-Time Clock interrupts are not supported.