## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### PRJINFO4 Field - ulExtendJobStatus

ulExtendJobStatus (ULONG) Extended job status flags.

Values are as follows:

Bit Description

0 PRJ4_INPRINTER - 0x00000001
Job in printer (0=No; 1=Yes)

1 PRJ4_STACKED - 0x00000002
Job is stacked (0=No; 1=Yes)

2 PRJ4_HELDINPRINTER - 0x00000004
Job held in printer (0=No; 1=Yes)

3 PRJ4_JOBSTARTED - 0x00000008
Job has begun printing (0=No; 1=Yes)

4 - 31 Reserved

This field can be set with SplSetJob using the PRJ_EXTENDSTATUSus.PARMNUM( 24) parameter.