## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### GreDeviceAnimatePalette Return Value - rc

rc (ULONG) - returns Return codes.

PAL-ERROR Error Count of the hardware palette slots changed.

Possible Errors Detected: When an error is detected, the handling routine must call WinSetErrorInfo to post the condition. Error codes for conditions that the handling routine is expected to check include:

PMERR_PALETTE_BUSY
PMERR_INV_IN_AREA
PMERR_INV_IN_PATH.