## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### BITMAPINFO

Bit-map information structure.

Each bit plane logically contains (cx * cy * cBitCount) bits, although the actual length can be greater because of padding.

See also BITMAPINFO2, which is preferred.

    typedef struct _BITMAPINFO {

      ULONG      cbFix;         /*  Length of fixed portion of structure. */

      USHORT     cx;            /*  Bit-map width in pels. */

      USHORT     cy;            /*  Bit-map height in pels. */

      USHORT     cPlanes;       /*  Number of bit planes. */

      USHORT     cBitCount;     /*  Number of bits per pel within a plane. */

      RGB        argbColor[1];  /*  Array of RGB values. */

    } BITMAPINFO;

    typedef   BITMAPINFO   * PBITMAPINFO ;