## Storage Device Driver Reference

[prev][next][parent][TOC]

### Installation

This CD-ROM contains the executables, libraries, grammars, and test cases necessary to run optical test suites.

The following procedure describes installation for running test cases:

1.Copy the component files from the Device Driver Kit for OS/2 CD-ROM to the hard drive. All files should reside in a common directory, such as \ TOPTICAL. If the target directory is C:\TOPTICAL and the E: drive contains the information from the Device Driver Kit for OS/2, then use the following commands to copy the optical test suite:

       [C:\]md toptical

       [C:\]cd toptical

       [C:\toptical]copy e:\ddk\testcert\storage\function\dasd\*

       [C:\toptical]copy e:\ddk\testcert\general\ddtt\*

2.Add C:\TOPTICAL to the LIBPATH and PATH in the CONFIG.SYS file.

3.Reboot your machine so the new LIBPATH entry takes effect.

The following DDTT files are required for execution of optical scripts:

DDTT.EXE

DDTT.DLL

GLOBAL.DLL

GLOBAL.GRA

DDTOPTI.DLL

OPTI.GRA