## Printer Device Driver

[prev][next][parent][TOC]

### stop_color_sorting()

Stops color sorting. This function is called at the end of a page and the end of a frame. Its basic operation is to replay the journal file and perform only those operations requiring the current pen. Thus, all drawing operations are completed for each pen in one operation, thereby reducing the number of (slow) pen change operations. This function processes the color sorting information and is called at the end of a page. This function will stop journaling, then play the journal file for each pen used in the carousel. It will set the current pen based on lightness to darkness for a given carousel. If an ABORTDOC signal is received, the bEnableOutput flag will be cleared, further output will cease (output_bytes will stop sending) , and the rest of the journal file replay will be skipped.