## MMPM/2 Device Driver Reference

[prev][next][parent][TOC]

### AUDIO_LOAD (44h) - Pointer to structure

Pointer to structure The data packet parameter is a pointer to the following data structure.

    typedef struct _load {
      CHAR FAR      *pbBuffer;
      ULONG          ulSize;
      ULONG          ulFlags;
    } MCI_AUDIO_LOAD;

    typedef   MCI _ AUDIO _ LOAD   FAR   * LPMCI _ AUDIO _ LOAD ;