## Display Device Driver Reference for OS/2

[prev][next][parent][TOC]

### Function 115h - Flags

Flags

Defined as follows:

    Bit 0 indicates whether the physical video

          buffer should be printed.

          OFF = Print only the contents of the logical

                video buffer.

          ON  = Print the contents of the physical

                video buffer, if appropriate.

    Bits 1-15 are reserved and must be OFF.