## MMPM/2 Device Driver Reference

[prev][next][parent][TOC]

### VCAI_CAPTURE_FORMAT (65h) - Pointer to structure

Pointer to structure The data packet parameter is a pointer to the following data structure.

    typedef struct _VCAIMAGECF {
      ULONG       ulFlags;
      ULONG       ulNumFormats;
      ULONG       ulCurIndex;
      ULONG       FourCC[64];
    } VCAIMAGECF;

    typedef   VCAIMAGECF   FAR   *   PVCAIMAGECF ;