## Storage Device Driver Reference

[prev][next][parent][TOC]

### CDROM_READ2352

Category 80h Function 72h - Read Long

This function reads 2352 bytes of each specified sector into the data buffer. Header and trailer data are read in addition to the 2048-byte data field. The number of sectors to read is passed as input. Address mode may be specified as either Redbook or Logical Block. SECTORSTART and TIMESTART parameters are mutually exclusive.