## MMPM/2 Device Driver Reference

[prev][next][parent][TOC]

### MCI_AUDIO_INIT Field - sDeviceID

sDeviceID (SHORT) If the call is successful, the type of device is returned in the sDeviceID field. The defined values used by sDeviceID are:

    MINIDD               0    /* Minimal device driver             */

    ACPA                 1    /* IBM ACPA                          */

    MACPA                2    /* IBM M-ACPA                        */

    MPU401               3    /* Roland MPU-401 or compatible      */

    SOUND_BLASTER        4    /* Creative Labs Sound Blaster       */

    IMF                  5    /* IBM Music Feature                 */

    PS1                  6    /* IBM Personal System/1 audio

                                 feature                           */

    PAS16                7    /* Media Vision ProAudio Spectrum 16 */

    DS201                9    /* DS201 audio adapter               */