## MMPM/2 Device Driver Reference

[prev][next][parent][TOC]

### VCAI_RESTORE_FORMAT (64h) - Pointer to structure

Pointer to structure The data packet parameter is a pointer to the following data structure.

    typedef struct _VCAIMAGERF {
      ULONG       ulFlags;
      ULONG       ulNumFormats;
      ULONG       ulCurIndex;
      ULONG       FourCC[64];
    } VCAIMAGERF;

    typedef   VCAIMAGERF   FAR   *   PVCAIMAGERF ;