## Storage Device Driver Reference

[prev][next][parent][TOC]

### SEEK (0Bh) and Seek (2Bh)

The SEEK (6 byte) and SEEK (10 byte) commands request that the logical unit seek to the specified logical block address.

The adapter device driver must complete the seek operation successfully even if the target sector is an audio sector. If a seek command to an audio sector is not supported by the drive, the driver should issue an alternative command which can successfully seek to the audio sector.