## Storage Device Driver Reference

[prev][next][parent][TOC]

### READ TOC (43h)

The READ TOC command requests that the target transfer data from the table of contents to the initiator.

For drives which do not support a READ TOC command while an audio play operation is in progress, the adapter device driver should buffer the entire TOC data when media is first mounted in the drive. This will ensure the TOC data is retrievable during an audio play operation.

All TOC data is returned in binary format.

Refer to the ANSI SCSI-2 specification for a detailed description of this command.