## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### GreExcludeClipRectangle Parameter - prclRect

prclRect (PRECTL) - input Pointer to rectangle in world or device coordinates.

RECTL structure:

xLeft Minimum x-coordinate of rectangle
yBottom Minimum y-coordinate
xRight Maximum x-coordinate of rectangle
yTop Maximum y-coordinate

All the boundaries of this rectangle are considered to be part of the interior and are clipped accordingly.