## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### SplRegister Parameter - pulHandle

pulHandle (PULONG) - in/out Pointer to spooler alert handle.

For initial registration, the value pointed to by this parameter should be 0 (zero). If an application wants to make better use of spooler resources, the application can use the same returned spooler handle for all of its alert registration.