## Input/Output Device Driver Reference

[prev][next][parent][TOC]

### Error Replacement Character Processing

The processing that the physical device driver performs when a received character has an error (parity, framing, overrun, or lack of receive queue space) is determined by whether Error Replacement Character Processing is enabled (active).

Initial Value Error replacement character processing is disabled.
First Level Open Error replacement character processing is disabled.
Mode Utility No effect.