## Physical Device Driver Reference

[prev][next][parent][TOC]

### ADJHANDLELIST Field - cMaxHandles

cMaxHandles (USHORT) Number of handles that can be accepted in the handles array. This field must be set by the caller.

The default ADJHANDLELIST provides room for one handle. In this case, cMaxHandles must be set to 1. Refer to the example in RMKeyToHandleList, if more than one Adjunct handle is expected.