## Input/Output Device Driver Reference

[prev][next][parent][TOC]

### Click-Lock Time

This value determines the time that is permitted to elapse between the time the coordinates first become locked and when normal X,Y reporting is resumed.

A large value makes double clicking a less hurried process but also makes immediate minor adjustments and close manipulation by dragging slightly more cumbersome.