## Physical Device Driver Reference

[prev][next][parent][TOC]

### PDSK_VERIFYPHYSTRACK (65h) - Command Information

Command Information A bit field as follows:

Bit 0 If clear (0), the track layout contains non-consecutive sectors or does not start with Sector 1. If set (1), the track layout starts with Sector 1 and contains only consecutive sectors.

All other bits are reserved and must be set to 0.