## Display Device Driver Reference for OS/2

[prev][next][parent][TOC]

### Procomm Plus

The following procedure explains how to test Procomm Plus:

1.Open an DOS full screen session (VDM) to run Procomm Plus. If you do not have Procomm Plus installed, refer to your Procomm Plus Installation Manual for instructions.

2.At the Procomm Plus screen, press [Enter] to go to terminal mode.

3.Press [Alt+D] for dial mode.

4.Type the number and start the call.

5.When the connection has been established perform login.

6.Type a "U" to upload a file or a "D" to download a file.

7.Type the modem protocol type. The most common protocols are Kermit, Xmodem and Ymodem. Use these protocols along with a mixture of the others.

8.Type the file name.

9.To begin the file transfer, press Page Down to download files or Page Up to upload files.

10.Verify that the file transfer has completed.

11.Send or receive at least three files changing modem types.

Note: Verify that video corruption does not occur in all operations.