## Display Device Driver Reference for OS/2

[prev][next][parent][TOC]

### Query Physical Buffer - Function 110h

Category:
Function:
110h
Description:
Query Physical Buffer

Select an item:

    Description
    Parameter Packet Format
    Returns
    Remarks

This function returns an LDT selector that can be used to access the physical video buffer. The current physical video buffer is returned unless a specific address range is requested.