## MMPM/2 Device Driver Reference

[prev][next][parent][TOC]

### MIX_SETCONTROL (64h) - Set State of a Mixer Line

Category:
AUDIO_IOCTL_CAT (80h)
Function:
MIX_SETCONTROL (64h)
Description:
Set State of a Mixer Line

Select an item:

    Description
    Parameter Packet Format
    Data Packet Format
    Returns
    Example Code

This IOCtl enables an application to set the current state of a particular line.