## MMPM/2 Device Driver Reference

[prev][next][parent][TOC]

### MIX_SETCONNECTIONS (61h) - Pointer to structure

Pointer to structure The data packet parameter is a pointer to the following data structure.

    typedef struct _LINECONNECTIONS {
      ULONG       ulLength;
      ULONG       ulConnections;
      ULONG       ulLine;
    } LINECONNECTIONS;

    typedef   LINECONNECTIONS   FAR   * PLINECONNECTIONS ;

The caller is responsible for filling in the ulLine and ulConnections fields of the LINECONNECTIONS structure.