## Using Your DDK

[prev][next][parent][TOC]

### Adapter Driver For ABIOS Floppy

Driver Description:

The ABIOS floppy adapter driver provides device support for diskette drives on Micro Channel systems.

Compilers/Assemblers Required:

           Microsoft MASM 5.1  (supplied with the DDK)
           Microsoft C 6.0

Build Instructions:

1.Set the environment variables so the correct tools are picked up during the build.

    e.g., SET PATH=<drive>:\DDK\TOOLS;%PATH%

Where <drive> represents your DDK installed drive and DDK represents the DDK installed directory. On the CD-ROM, the TOOLS directory path is DDK\ TOOLS.

2.Before the FIRST build is attempted, run (only once) the COPYC60.CMD REXX command file in the DDK\TOOLS directory. This command copies the set of needed files from your copy of the Microsoft C 6.0 compiler to the proper directories under the DDK base directory.

    e.g., COPYC60 <MSCdrive>:\'MSC60' <drive>:\DDK

Where <MSCdrive> represents the Microsoft C 6.0 installed drive and 'MSC60' represents the Microsoft C 6.0 installed directory, <drive> represents your DDK installed drive and DDK represents the DDK installed directory.

To build the Adapter Driver for ABIOS Floppy:

3.Change the directory to DDK\BASE\SRC\DEV\DASD\IBM\IBM2FLPY.

4.Invoke NMAKE on the resident makefile.

Files Created by Successful Build:

         Directory:  \DDK\BASE\SRC\DEV\DASD\IBM\IBM2FLPY

         o  IBM2FLPY.ADD