## Physical Device Driver Reference

[prev][next][parent][TOC]

### RMDevIDToHandleList - Calling Parameters

IDType (IDTYPE) - input The type of device ID. The following values are valid:

RM_IDTYPE_RM Internal to Resource Manager.

RM_IDTYPE_EISA EISA (also used for ISA PNP).

RM_IDTYPE_PCI PCI device IDs.

RM_IDTYPE_LEGACY Legacy device ID not defined by Intel.

DeviceID (DEVID) - input Uniquely identifies the particular device or adapter.

FunctionID (DEVID) - input Uniquely identifies a function located on a multi-function adapter.

CompatibleID (DEVID) - input Provides the device IDs of other compatible devices.

VendorID (VENDID) - input Provides the vendor ID for the device.

SerialNumber (SERNUM) - input Provides the serial number for the device.

SearchFlags (ULONG) - input Indicates the type of search to be executed. The following combination of searches are valid:

SEARCH_ID_DEVICEID Search on adapter ID only.

SEARCH_ID_FUNCTIONID Search on function ID only.

SEARCH_ID_COMPATIBLEID Search on compatible ID only.

hStartNode (HDETECTED) - input The handle of the Resource Manager node at which to start the search. The following pseudohandles are supported:

HANDLE_PREVIOUS_DETECTED Previously detected nodes.

HANDLE_CURRENT_DETECTED Current detected nodes.

pHndList (PHANDLELIST) - output Pointer to array of detected handles that match the detected IDs.

rc (APIRET) - returns On systems where the Resource Manager driver is not installed, the library interface code will return RMRC_NOT_INSTALLED.

RMRC_BAD_DETECTHANDLE
RMRC_INVALID_PARM_VALUE
RMRC_NULL_POINTER
RMRC_SUCCESS