## Using Your DDK

[prev][next][parent][TOC]

### 32-Bit Plotter Presentation Device Driver

Driver Description:

The Plotter device driver is a 32-bit presentation device driver based on the IBM plotter language.

Compilers/Assemblers Required:

         Microsoft MASM 5.1      (supplied with the DDK)
         IBM VisualAge C++ V3.0

Build Instructions:

1.Ensure the necessary compilers and assemblers are installed.

2.Run the SETCMPLR.CMD REXX command file located in the DDK\TOOLS directory. This command initializes environment variables to be used during the build.

e.g., SETCMPLR <MSCpath> <VACpath> <CSETpath> <DDKpath>

    Where <MSCpath> represents the Microsoft C 6.0 install directory
           <VACpath> represents the IBM VisualAge C++ install directory
           <CSETpath> represents the IBM C Set ++ install directory
           <DDKpath> represents the DDK install directory

Note: A period (.) may be substituted for a compiler directory that is not used during the build.

3.Change the directory to DDK\PRINT\SRC\OSDD\PLOTTER.

4.To build the retail version, invoke NMAKE specifying the RETOS2C parameter on the resident makefile.

To build the debug version, invoke NMAKE specifying the DBGOS2C parameter on the resident makefile.

Files Created by Successful Build:

         Retail Version:
         Directory:  \DDK\PRINT\REL\OS2C\RETAIL\EN\OS2\DRIVERS\PLOTTERS

         o  PLOTTERS.DRV

         Debug Version:
         Directory:  \DDK\PRINT\REL\OS2C\DEBUG\EN\OS2\DRIVERS\PLOTTERS

         o  PLOTTERS.DRV