## Using Your DDK

[prev][next][parent][TOC]

### DBCS ISA/EISA 16-Bit Floppy Driver

Driver Description:

The ISA/EISA floppy device driver is the diskette driver for ISA/EISA bus systems.

Compilers/Assemblers Required:

         Microsoft MASM 5.1  (supplied with the DDK)
         Microsoft C 6.0

Build Instructions:

1.Run the SETDBCS.CMD command file in the <drive>:\DDK\TOOLS directory, passing <drive> and DDK as parameters. This will set the path and environment variables.

    e.g., SETDBCS <drive>:\DDK

Where <drive> represents your DDK installed drive and DDK represents the DDK installed directory. On the CD-ROM, the TOOLS directory path is DDK\ TOOLS.

2.Before the FIRST build is attempted, run (only once) the COPYC60.CMD REXX command file in the DDK\TOOLS directory. This command copies the set of needed files from your copy of the Microsoft C 6.0 compiler to the proper directories under the DDK base directory.

    e.g., COPYC60 <MSCdrive>:\'MSC60' <drive>:\DDK

Where <MSCdrive> represents the Microsoft C 6.0 installed drive and 'MSC60' represents the Microsoft C 6.0 installed directory, <drive> represents your DDK installed drive and DDK represents the DDK installed directory.

3.Change the directory to DDK\DBCS\SRC\DEV\DASD\IBM\IBM1FLPY.

4.Invoke NMAKE on the resident makefile.

Files Created by Successful Build:

         Directory:  \DDK\DBCS\SRC\DEV\DASD\IBM\IBM1FLPY

         o  IBM1FLPY.ADD