## MMPM/2 Device Driver Reference

[prev][next][parent][TOC]

### VCAI_VIDEOADJ (75h) - Remarks

When setting a value, put the value desired (in the range of 0 to 255) into the value's field. If resetting the value to the defaults, put DEFAULT into the value's field. If no change is desired for a particular value, put NO_ CHANGE in the value's field. The call always returns the current value or NOT_SUPPORTED for each setting after the value has been updated.