## MMPM/2 Device Driver Reference

[prev][next][parent][TOC]

### MIX_SETCONNECTIONS (61h) - Connect an Input Line to an Output Line

Category:
AUDIO_IOCTL_CAT (80h)
Function:
MIX_SETCONNECTIONS (61h)
Description:
Connect an Input Line to an Output Line

Select an item:

    Description
    Parameter Packet Format
    Data Packet Format
    Returns
    Example Code

This IOCtl enables an application to connect an input line to an output line.