## Storage Device Driver Reference

[prev][next][parent][TOC]

### PAUSE/RESUME (4Bh)

The PAUSE RESUME command requests that the device stop or start an audio play operation.

It shall not be considered an error to request a pause when a pause is already in effect or to request a resume when a play operation is in progress.

Refer to the ANSI SCSI-2 specification for a detailed description of this command.