## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### PRQINFO6 Field - uPriority

uPriority (USHORT) Queue priority.

The range is 1 through 9, with 1 being the highest queue priority.

The default job priority (DefJobPrio) is determined from:
DefJobPrio=100-(10* uPriority).

If a job is added with PRJ_NO_PRIORITY specified, DefJobPrio is used. If a default priority higher than the default job priority is specified, the default job priority is used. If a default priority lower than the default is specified, the specified job priority is used.

PRQ_DEF_PRIORITY Default priority
PRQ_MAX_PRIORITY Highest priority
PRQ_MIN_PRIORITY Minimum priority
PRQ_NO_PRIORITY No priority.