## Physical Device Driver Reference

[prev][next][parent][TOC]

### TOUCH_DEVDEP_SETTOUCHTHRESHOLD (56h) - Push hysteresis threshold

Push hysteresis threshold Sets the value of Z, when Z is decreasing on the chosen Z scale, at which the Touch display resets the selection detection bit in the status returned by Function 53h.

Note: Any parameter value of -1 causes the driver default value to be substituted.