## MMPM/2 Device Driver Reference

[prev][next][parent][TOC]

### Step 2

To create the stream, select Data Stream. Select SpiCreate to display the Create Data Stream window. [Artwork not shown]

Enter the input source and target stream handler IDs. For example, enter the FSSH source ID (4) and the AUDIOSH$ target ID (2). Select a stream data type, and select OK.

The Stream State field in the Active Streams window displays information about the stream that has been created. The audio device driver has accepted the audio IOCtls and the IDC APIs to create the stream.