## MMPM/2 Device Driver Reference

[prev][next][parent][TOC]

### VSD_RESTORE - Example Code

The following code illustrates how to activate an audio VSD using VSD_ RESTORE.

       ULONG   rc;

       HVSD    hvsd;

           rc = pInstance->pfnAUDIOIF( hvsd,

                                       VSD_RESTORE,

                                       0L,

                                       0 );

           return(rc)