## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### GreSetGraphicsField - Parameters

hdc (HDC) - input Device context handle.

prclGraphicsField (PRECTL) - input Pointer to graphics field.

RECTL structure:

xLeft Minimum x-coordinate of graphics field
yBottom Minimum y-coordinate
xRight Maximum x-coordinate of graphics field
yTop Maximum y-coordinate

An error is raised when xLeft is greater than xRight, or yBottom is greater than yTop.

pInstance (PVOID) - input Pointer to instance data.

lFunction (ULONG) - input High-order WORD=flags; low-order WORD= NGreSetGraphicsField.

fSuccess (BOOL) - returns Return codes.

This function returns BOOLEAN (fSuccess).

TRUE Successful
FALSE Error

Possible Errors Detected: When an error is detected, the handling routine must call WinSetErrorInfo to post the condition. Error codes for conditions that the handling routine is expected to check include:

PMERR_HDC_BUSY
PMERR_INV_COORDINATE
PMERR_INV_GRAPHICS_FIELD
PMERR_INV_HDC
PMERR_INV_IN_AREA
PMERR_INV_IN_PATH

Refer to the "Error Explanations" section in the Presentation Manager Programming Reference for further explanation.