## MMPM/2 Device Driver Reference

[prev][next][parent][TOC]

### VSD_QUERYSTATUSLEVEL - Syntax

This subcommand of the VSD_QUERY command queries the status of the audio input level (percentage). This command is optional.

This command is sent using VSDEntry as follows:

        VSDEntry(hvsd, ulFunc, ulFlags, pRequest)

hvsd (HVSD) Handle to a VSD.

ulFunc (ULONG) Set to VSD_QUERY.

ulFlags (ULONG) Set to VSD_QUERYSTATUSLEVEL.

pRequest (PULONG) Current level of device.

rc (ULONG) Error code indicating success or the type of failure:

VSDERR_SUCCESS The command was successful.