## Pen for OS/2 Device Driver Reference

[prev][next][parent][TOC]

### Reset Trace Table - Function 52h

Category 90h, Driver IOCtls - Reset Trace Table

Select an item:

    Description
    Parameter Packet Format
    Data Packet Format

    #define PEN_FUNC_RTT 0x052

This function resets the transaction trace buffer. Resetting the trace buffer is a convenient way to view only current stroke data.