## MMPM/2 Device Driver Reference

[prev][next][parent][TOC]

### VSD_SETMIXCONNECTIONS - Example Code

The following code illustrates how to route the output of a connector to the internal mixer circuitry.

      LINECONNECTIONS   mixinfo;

      mixinfo.ulLine = SOURCE_SYNTHESIZER;

      mixinfo.ulConnection = SINK_SPEAKER;

      rc = pInstance->((HVSD)pInstance->hvsd,

                       VSD_SET,

                       VSD_SETMIXCONNECTIONS,

                       (PVOID)&mixinfo);

      return(rc);