## Presentation Device Driver Reference for OS/2

[prev][next][parent][TOC]

### PrtResetAbort

Select an item:

    Syntax
    Parameters
    Returns
    Remarks
    Glossary

Description:

PrtResetAbort resets an aborted print job to allow a print driver to send multiple reset sequences to the printer. After PrtResetAbort is called successfully, the print driver can issue PrtWrite for this device handle

    #define INCL_SPL

    #define INCL_SPLDOSPRINT

    #include <os2.h>

    HFILE    hDevice;  /*  The device handle returned by PrtOpen. */

    ULONG    rc;       /*  Return codes. */

    rc = PrtResetAbort(hDevice);