## Physical Device Driver Reference

[prev][next][parent][TOC]

### TOUCH_DEVINDEP_GETSELECTMECH (62h) - Type

Type The field in which the selection detection flat (bit) in the status word returned in Function 66h is set or reset.

Bit 0

0 Push harder (default)

1 Lift off

Bit 1

0 First value taken

1 Single-touch algorithm applied

Bit 2

0 First value taken

1 Stable-region algorithm active

Bit 3-F

0 Reserved.